Stepper Motor 1.8 deg/step

Remote Controller

Has a receiver/transmitter and PLC for establishing communication protocol and logging data

Contains SD Card

12V 8Ah Battery

Lead-Acid

10RPM Geared Motor

Motor Drive

Arduino BLT7960

PLC Microcontroller

(FubarinoSD)

HMI

LiquidCrystal Display

Transmitter/Receiver

